

5V



1000 uF

I2C Clock

I2C Data

Pixel Data Nose

Pixel Data Mouth



P3

P2

P1

P0

Propeller Quick Start Board



3.3V

5V